

**RISK ASSESSMENT FINDINGS**

|  |  |
| --- | --- |
| **Department/Service** |  |
| **Date** |  |
| **Assessor** |  |
| **Approved By** |  |
| **Review Date** |  |

**Relevant Legislation:**

The Management of Health and Safety at Work Regulations 1999

**RISK ASSESSMENT RECORD**

**ACTIVITY and/or ENVIRONMENT TO BE ASSESSED: Painting and Decorating – Vocational education**

**DATE:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **KEY (People at risk)** | **Likelihood (L)** | **Severity (S)** | **Risk Calculation** | **Risk Rating** |
| E = Employee YP = Young Persons  P = Public  C = Contractors  V = Visitors  EM = Expectant Mothers | 1. Very Low (rare/very unlikely)  2. Low (unlikely)  3. Medium (could occur/possible)  4. High (likely to occur/probable)  5. Very High (near certain to occur) | 1. Insignificant (nuisance/discomfort)  2. Minor (no lost time)  3. Moderate (time loss)  4. Significant (serious/incapacity to work)  5. Major (Death) | Likelihood x Severity  =  Rating | **1- 6** **LOW RISK** Monitor   * 1. **MEDIUM RISK** Monitor, review & reduce risk where possible   **14-25** **HIGH RISK** Further Action Required |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1.Hazards Identified and potential harm it could cause** | **2. People**  **At Risk** | **3.Controls in Place** | **4.Risk Rating** | | | | **5. Further Action Required/ Recommendations** | **6.Target Date for Completion** |
| **L** | **S** | **Score** | **Risk** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Working at Height |  | See generic working at height risk assessment |  |  |  |  |  |  |
| Manual Handling |  | See generic manual handling risk assessment |  |  |  |  |  |  |
| Sanding down woodwork etc. before painting |  | * All staff to wear respiratory protection when sanding down old painted surfaces, woodwork, metal work etc. * All dusts to be dampened down before sweeping up. |  |  |  |  |  |  |
| Moving about in general |  | * Floor surfaces to be kept in a good clean condition. * Spilled paint and liquids will be cleaned up immediately. * Work areas to be cordoned off to prevent access by other people. |  |  |  |  |  |  |
| Use of flammable materials such as paint thinners etc. |  | * Flammable liquids to be kept to a minimum on site and kept locked in a flameproof cabinet when not in use. * Naked flames (e.g. from blow lamps etc.) to be kept away from the area where flammable liquids are being used/stored. * Staff to be made aware of fire prevention methods associated with their work. * All rags and cleaning cloths used with flammable liquids to be placed in a flameproof, lidded container after use. * Containers to be kept away from naked flames. * All such rags and cleaning cloths etc. to be disposed of properly. |  |  |  |  |  |  |
| Using paints and varnishes etc. |  | * Where possible, paints and varnishes etc. of a non-hazardous type to be used. * Staff to be instructed to read the safety label on all paint and varnish etc. containers before use. * Where a substance is identified as hazardous, COSHH assessment to be carried out and specific control measures introduced. * Staff / pupils to wear the relevant personal protective equipment when carrying out painting tasks, including coveralls, gloves, eyeshields etc. * All splashes on the skin to be treated immediately. |  |  |  |  |  |  |
| Use of cutting tools during wallpapering |  | * Staff to use decorator’s scissors for cutting wallpaper. * The use of knives by pupils to be prohibited/closely supervised. |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |